REAR MOUNT CAMERA REMOVAL/INSTALLATION

id092000805900

1. Disconnect the negative battery cable.

2. Remove the liftgate upper trim. (See LIFTGATE UPPER TRIM REMOVAL/INSTALLATION.)

3. Remove the liftgate side trim. (See LIFTGATE SIDE TRIM REMOVAL/INSTALLATION.)

4. Remove the liftgate lower trim. (See LIFTGATE LOWER TRIM REMOVAL/INSTALLATION.)

5. Remove the rear finisher. (See REAR FINISHER REMOVAL/INSTALLATION.)

6. Remove in the order indicated in the table.

ac9uuw00000416

1 | Screw
2 | Rear mount camera

7. Install in the reverse order of removal.