NO. 4 MIL ILLUMINATES [INSTRUMENT CLUSTER]

id0903d5807700

4 | MIL illuminates
--- | ---
POSSIBLE CAUSE | • PCM malfunction • Instrument cluster malfunction • Connector or pin malfunction • Short circuit in wiring harness between CAN-L, CAN-H and ground • Open circuit in CAN wiring harness (CAN-L, CAN-H) • CAN wiring harness (CAN-L, CAN-H) short each other

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Start the engine. • Does the MIL turn off? | Yes | Troubleshooting completed.
No | Go to the next step.
2 | • Inspect the DTC for the instrument cluster ON-BOARD DIAGNOSTIC SYSTEM. • Have DTCs U2064 or U2023 been recorded in memory? | Yes | Inspect the DTC for the PCM. (See ON-BOARD DIAGNOSTIC TEST [MZI-3.7].)
No | Go to the next step.
3 | • Disconnect the negative battery cable. • Measure the resistance between the DLC-2 terminals F and E. • Is the resistance below 60 ohms? | Yes | Go to the next step.
No | Go to Step 5.
4 | • Inspect the DLC-2 terminals F and E for short to power supply or ground. • Is there any malfunction? | Yes | Inspect the wiring harness and CAN system-related module. Repair or replace the malfunctioning part.
No | Replace the instrument cluster.
5 | • Turn the ignition switch to the OFF position. • Inspect the instrument cluster connector terminals for poor connection (such as damaged/pulled-out pins, and corrosion). • Are the terminals normal? | Yes | Go to the next step.
No | Repair or replace the terminal.
6 | • Disconnect the negative battery cable. • Measure the resistance between the instrument cluster connector terminals 1W and 1X. • Is the resistance 114—126 ohms? | Yes | Inspect the wiring harness and CAN system-related module. Repair or replace the malfunctioning part.
| No | Replace the instrument cluster.