FRONT SASH MOLDING REMOVAL

id091600805000

  Warning
  • Using a razor with bare hands can cause injury. Always wear gloves when using a razor.

1. Remove the power outer mirror. (See POWER OUTER MIRROR REMOVAL/INSTALLATION.)

2. Press tab A in the direction of the arrow and remove it.

ac9uuw00002048

3. While cutting the double-sided adhesive tape using a flathead screwdriver or a razor, separate the front sash molding from the body.

4. Rotate the front sash molding at the pivot of tab B in the direction of arrow D and remove it.

5. Remove the tab C.

6. Remove the front sash molding.