POWER LIFTGATE (PLG) CONTROL MODULE REMOVAL/INSTALLATION

id091100000900

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Trunk box (See TRUNK BOX REMOVAL/INSTALLATION.)

  (2) Seat side box (LH) (See SEAT SIDE BOX REMOVAL/INSTALLATION.)

  (3) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (4) Third-row seat (See THIRD-ROW SEAT REMOVAL/INSTALLATION.)

  (5) Third-row seat belt lower anchor installation bolt (LH) (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (6) Trunk side trim (LH) (See TRUNK SIDE TRIM REMOVAL/INSTALLATION)

3. Disconnect the PLG control module connector.

4. Remove the bolts.

ac9wzw00001038

5. Remove the PLG control module.

6. Install in the reverse order of removal.