THIRD-ROW SEAT BELT REMOVAL/INSTALLATION

id081100802600

  Caution
  • The ELR (emergency locking retractor) has a spring that will unwind if the retractor cover is removed. The spring cannot be rewound by hand. If this occurs, the ELR will not work properly. Therefore, do not disassemble the retractor.

1. Remove the following parts:

  (1) Trunk box (See TRUNK BOX REMOVAL/INSTALLATION.)

  (2) Seat side box (See SEAT SIDE BOX REMOVAL/INSTALLATION.)

  (3) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (4) Third-row seat (See THIRD-ROW SEAT REMOVAL/INSTALLATION.)

2. Remove the bolt A.

ac9wzw00000954

3. Remove the rear scuff plate inner. (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)

4. Remove the trunk side trim. (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

5. Remove the cover.

6. Remove the bolt B.

7. Remove the third-row seat belt.

8. Install in the reverse order of removal.