ADVANCED KEY CONSTRUCTION

id091400596800

• A maximum of six transmitters can be programmed for one vehicle.
• A built-in operation indicator light illuminates according to the button operation.
• In case the transmitter is inoperable due to battery depletion, the doors can be locked/unlocked and the engine can be started using the auxiliary key.
• A transponder is built into the auxiliary key.
• An intruder sensor cancel button has been installed on the advanced key. If the intruder sensor cancel button is on while the theft-deterrent system is pre-armed, intruder sensor ultrasonic wave output is cut, and movement detection is stopped.

ac9wzn00000303