INBOARD LIGHT REMOVAL/INSTALLATION

id091800806100

1. Disconnect the negative battery cable.

2. Remove the service hole cover.

ac9wzw00002572

3. Remove in the order indicated in the table.

ac9wzw00001758

1 | Connector
2 | Nut
3 | Bracket
4 | Inboard light (See Inboard Light Installation Note.)

4. Install in the reverse order of removal.

Inboard Light Installation Note

1. Insert the inboard light into the liftgate as shown in the figure, pivot it inward and then fix in place.

ac9uuw00002065

2. Push the bracket onto the liftgate as shown in the figure and install.

ac9uuw00000607