FRONT SCUFF PLATE REMOVAL/INSTALLATION

id091700801400

Front Scuff Plate Inner

1. Pull the front scuff plate inner upward while detaching tab A, detach clips B, pins C, and tab D, from the body, and then remove the front scuff plate inner.

ac9uuw00000401

2. Install in the reverse order of removal.

Front Scuff Plate Outer

1. Pull the front scuff plate outer upward, detach clips A, tabs B, and pin C, from the body, and then remove the front scuff plate outer.

ac9uuw00000402

2. Install in the reverse order of removal.