FRONT DOOR SPEAKER REMOVAL/INSTALLATION

id092000802200

1. Disconnect the negative battery cable.

2. Remove the inner garnish. (See INNER GARNISH REMOVAL/INSTALLATION.)

3. Remove the front door trim. (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

ac9wzw00001233

1 | Screw
2 | Front door speaker (See Front Door Speaker Installation Note.)
3 | Connector

5. Install in the reverse order of removal.

Front Door Speaker Installation Note

1. Remove the speaker with the wiring harness passing through the groove of the front door module.

ac9uuw00002221

  Caution
  • If the speaker is installed with the wiring harness out of the groove, an open circuit in the wiring harness could occur.