ANTENNA FEEDER NO.1 REMOVAL/INSTALLATION

id092000812200

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)

  (2) Front console box mat (See FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION.)

  (3) Indicator panel (See INDICATOR PANEL REMOVAL/INSTALLATION.)

  (4) Front console box (See FRONT CONSOLE BOX REMOVAL/INSTALLATION.)

  (5) Dashboard under cover (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

  (6) Side wall (See SIDE WALL REMOVAL/INSTALLATION.)

  (7) Console panel (See CONSOLE PANEL REMOVAL/INSTALLATION.)

  (8) Console cover (See CONSOLE COVER REMOVAL/INSTALLATION.)

  (9) Console (See CONSOLE REMOVAL/INSTALLATION.)

  (10) Front scuff plate inner (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)

  (11) Front side trim (See FRONT SIDE TRIM REMOVAL/INSTALLATION.)

  (12) Glove compartment (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)

  (13) Bonnet release lever (See BONNET LATCH AND RELEASE LEVER REMOVAL/INSTALLATION.)

  (14) Fuel-filler lid release lever (R.H.D.) (See FUEL-FILLER LID OPENER REMOVAL/INSTALLATION.)

  (15) Lower panel (See LOWER PANEL REMOVAL/INSTALLATION.)

  (16) Column cover (See COLUMN COVER REMOVAL/INSTALLATION.)

  (17) Driver-side air bag module (See DRIVER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

  (18) Steering wheel (See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)

  (19) Combination switch (See COMBINATION SWITCH REMOVAL/INSTALLATION.)

  (20) Center panel (See CENTER PANEL REMOVAL/INSTALLATION.)

  (21) Meter hood (See METER HOOD REMOVAL/INSTALLATION.)

  (22) Instrument cluster (See INSTRUMENT CLUSTER REMOVAL/INSTALLATION.)

  (23) Audio unit (with audio system) (See AUDIO UNIT REMOVAL/INSTALLATION.)

  (24) Car-navigation unit (with car-navigation system) (See CAR-NAVIGATION UNIT REMOVAL/INSTALLATION.)

  (25) Steering shaft (See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)

  (26) A-pillar trim (See A-PILLAR TRIM REMOVAL/INSTALLATION.)

  (27) Side panel (See SIDE PANEL REMOVAL/INSTALLATION.)

3. Disconnect the front door wiring harness connector (Driver side). (SeeFRONT DOOR MODULE PANEL REMOVAL/INSTALLATION.)

4. Disconnect the dashboard harness connectors.

5. Remove the brake switch from the brake pedal with the brake switch connector connected. (See BRAKE PEDAL REMOVAL/INSTALLATION [L.H.D.].) (See BRAKE PEDAL REMOVAL/INSTALLATION [R.H.D.].)

6. Remove the selector lever component. (See SELECTOR LEVER COMPONENT REMOVAL/INSTALLATION.)

7. Remove the windshield wiper arm and blade. (See WINDSHIELD WIPER ARM AND BLADE REMOVAL/INSTALLATION.)

8. Remove the cowl grille. (See COWL GRILLE REMOVAL/INSTALLATION.)

9. Remove the windshield wiper motor. (See WINDSHIELD WIPER MOTOR REMOVAL/INSTALLATION.)

10. Remove in the dashboard. (See DASHBOARD REMOVAL/INSTALLATION.)

11. Remove in the clip A, B, and C.

12. Remove in the antenna feeder No.1.

13. Install in the reverse order of removal.

L.H.D.

ac9wzw00001068

R.H.D.

ac9wzw00001069