DRIVE BELT CONSTRUCTION [MZI-3.7]

id0110c5102500

Generator and A/C Drive Belt

• A V-ribbed drive belt is employed.
• A drive belt auto tensioner with an embedded coil spring has been adopted to automatically maintain optimal drive belt tension.

ac9wzn00000681

Power Steering Oil Pump Drive Belt

• A V-ribbed drive belt is employed.
• For the removal/installation of the power steering oil pump drive belt, rotate the crankshaft using the SST and remove/install.

ac9wzn00000682