FRONT AUTO LEVELING SENSOR REMOVAL/INSTALLATION

id091800809800

1. Disconnect the negative battery cable.

2. Jack up the vehicle.

3. Remove the splash shield (LH).

4. Disconnect the connector.

ac9wzw00001264

5. Remove the nut and bolt.

6. Remove the front auto leveling sensor.

7. Install in the reverse order of removal.

8. Perform the auto leveling system initialization. (See AUTO LEVELING SYSTEM INITIALIZATION.)