DTC INSPECTION [POWER LIFTGATE (PLG) SYSTEM]

id0902e9345400

  Caution
  • Some of the PLG system DTCs cannot be stored unless the PLG system is operated. Therefore, always operate the PLG system before performing the DTC inspection.

1. Connect the M-MDS to the DLC-2.

ac9wzw00001083

2. After the vehicle is identified, select the following items from the initialization screen of the M-MDS.

  1. Select “Self Test”.
  2. Select “Modules”.
  3. Select “LTM”.

3. Verify the DTC according to the directions on the screen.

  • If any DTCs are displayed, perform troubleshooting according to the corresponding DTC inspection.

4. After completion of repairs, clear all DTCs stored in the PLG control module. (See CLEARING DTC [POWER LIFTGATE (PLG) SYSTEM].)