INSTRUMENTATION/DRIVER INFO. OUTLINE

id092200196800

• An LCD has been adopted to the instrument cluster which displays the trip computer, and odometer/tripmeter. (Without forward sensing camera (FSC))
• An LCD has been adopted to the instrument cluster which displays the trip computer, odometer/tripmeter and FOW/LDWS system operation display. (With FSC)
• The information display, which includes the clock (with click display), and A/C system displays, has been placed in the center of the instrument panel. It also includes the drive information system, depending on the vehicle grade.
• A trumpet-type horn with spiral, resonant pipes, has been adopted.
• A blind spot monitoring (BSM) system has been adopted. (With blind spot monitoring (BSM) system)
• A blind spot monitoring (BSM) system with a rear crossing traffic alert (RCTA) function has been adopted. (With blind spot monitoring (BSM) control module connector 10-pin type)
• A parking sensor system has been adopted. (With parking sensor system)
• A lane departure warning system (LDWS) has been adopted. (With FSC)
• A forward obstruction warning (FOW) system has been adopted. (With FSC)