CAMSHAFT POSITION (CMP) SENSOR REMOVAL/INSTALLATION [MZI-3.7]

id0140c3801500

1. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].)

2. Remove the battery. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].)

3. Remove the following parts for easier access:

  • MAF/IAT sensor connector
  • Vacuum hose (to master back) (See QUICK RELEASE CONNECTOR (EMISSION SYSTEM) REMOVAL/INSTALLATION [MZI-3.7].)
  • Resonance chamber and air cleaner assy (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [MZI-3.7].)

4. Disconnect the CMP sensor connector.

5. Remove the CMP sensor.

ac9wzw00001731

  Note
  • Lubricate the CMP O-ring seal with clean engine oil.

6. Install in the reverse order of removal.