DTC 96

id070200805100

DTC 96 | Rear airflow mode actuator (motor lock) (past)
--- | ---
POSSIBLE CAUSE | • Rear airflow mode actuator malfunction • Rear A/C unit (airflow mode links and/or airflow mode cranks) malfunction • Open or short circuit between rear airflow mode actuator and front climate control unit

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Disconnect rear airflow mode actuator connector. • Connect battery positive voltage to terminal F (or terminal G) and ground to terminal G (or terminal F) of rear airflow mode actuator connector. • Does rear airflow mode actuator operate? | Yes | Connect rear airflow mode actuator connector, then go to Step 3.
No | Go to the next step.
2 | • Remove rear airflow mode actuator. (See REAR AIRFLOW MODE ACTUATOR REMOVAL/INSTALLATION.) • Operate airflow mode main link by hand. • Does airflow mode main link operate smoothly? | Yes | Replace rear airflow mode actuator.
No | Replace airflow mode links and/or airflow mode cranks.
3 | • Disconnect front climate control unit connector (24-pin). • Connect battery positive voltage to terminal 1J (or terminal 1L) and ground to terminal 1L (or terminal 1J) of front climate control unit connector (24-pin). • Does rear airflow mode actuator operate? | Yes | Inspect the connection of the front climate control unit connector.
No | Repair wiring harness.