POSITION MEMORY CONTROL SYSTEM FUNCTION

id091300959300

Position Memory Detection Function

• Position memory control module detects the motor position (seat and outer mirror position) according to the pulse signal from the position sensors installed to each motor.

Position Memory Function

• One seat position for each memory switch, and one seat position for each transmitter can be programmed to the position memory control module.The number of memory switches and transmitters which can be programmed to the position memory control module is as follows:

  ― Memory switches: Three maximum
  ― Transmitters (Advanced keyless type): Six maximum
  ― Transmitters (Keyless entry type): Three maximum

• Programming of the seat position and outer mirror are possible according to the following procedures.

Seat position switch
  1. Slide the seat and move the outer mirror glass manually to the desired position.
  2. Press the set switch while pressing memory switches 1, 2, or 3.
  3. Buzzer sounds and the seat position is programmed.

Transmitter
  1. Slide the seat and move the outer mirror glass manually to the desired position.
  2. Press the UNLOCK button on the transmitter while pressing the set switch.
  3. Buzzer sounds and seat position is programmed.

  Note
  • Memory operation is possible when all of the following three conditions are met.
    ― Memory call up operation has not been performed.
    ― Manual operation has not been performed.
    ― When the vehicle is stopped (vehicle speed 3 km/h [2 mph] or less).

• Memory is reprogrammed when the seat position and outer mirror position are added to the memory switch which has already been programmed.
• If the negative battery cable is disconnected and 5 s or more have elapsed, all of the seat position and outer mirror position memory will be erased.

Memory Call Up Function (Memory Switch)

• Call up operation is performed which slides the seat and move the mirror to the programmed position by the memory switch operation.
Auto call up
• If the following conditions are met, the seat position and outer mirror position are automatically called up by the memory switch operation.

  ― Door is open (door switch on).
  ― Seat position has been programmed by memory switch.
  ― Outer mirror position has been programmed by memory switch.
  ― Memory switch and set switch are off.
  ― Ignition switch is in the OFF position.
  ― When the vehicle is stopped (vehicle speed 3 km/h [2 mph] or less).
    Note
    • Auto call up continues when the door is closed (door switch off) or the ignition switch is turned to the ON position during the auto call up.
    • Auto call up is cancelled when any of the following conditions are met during the auto call up.
      ― Manual operation using the power seat switch has been operated
      ― Manual operation using the power outer mirror switch has been operated
      ― Memory switch or set switch has been operated
      ― LOCK/UNLOCK operation has been performed using the transmitter with the ignition switch in the OFF position.
      ― While driving (vehicle speed 3 km/h [2 mph] or more).

Manual call up
• When the following conditions are met, the call up operation is performed only while the memory switch is being operated.

  ― Door is closed (door switch off) or the ignition switch is in the ON position.
  ― Seat position has been programmed.
  ― Outer mirror position has been programmed.
  ― Memory switch and set switch are off.
  ― When the vehicle is stopped (vehicle speed 3 km/h [2 mph] or less).
    Note
    • Auto call up is cancelled when any of the following conditions are met during the manual call up.
      ― Memory switch operation has stopped.
      ― Manual operation using the power seat switch has been performed.
      ― Manual operation using the power outer mirror switch has been performed.
      ― LOCK/UNLOCK operation has been performed using the transmitter with the ignition switch in the OFF position.
      ― While driving (vehicle speed 3 km/h [2 mph] or more).

Memory Call Up Function (Transmitter)

• If the door is opened within approx. 40 ±10 s after the doors are unlocked using the transmitter, the call up operation is performed and the seat moves to the position programmed in the transmitter.
• Seat position and outer mirror position are automatically called up when the following conditions are met.

  ― Seat position has been programmed by transmitter.
  ― Outer mirror position has been programmed by transmitter.
  ― Ignition switch is in the OFF position.
  ― Memory switch and set switch are off.
  ― When the vehicle is stopped (vehicle speed 3 km/h [2 mph] or less).
    Note
    • Auto call up continues when the door is closed (door switch off) or the ignition switch is turned to the ON position during the auto call up.
    • Auto call up is cancelled if any of the following conditions are met during the auto call up.
      ― Manual operation using the power seat switch has been performed.
      ― Manual operation using the power outer mirror switch has been performed.
      ― Memory switch or the set switch has been operated.
      ― LOCK/UNLOCK operation using the transmitter has been performed with the ignition switch in the OFF position.
      ― While driving (vehicle speed 3 km/h [2 mph] or more)