PARKING SENSOR BUZZER INSPECTION

id092200024000

1. Disconnect the negative battery cable.

2. Remove the dashboard under cover (Driver side). (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

3. Remove the parking sensor buzzer. (See PARKING SENSOR BUZZER REMOVAL/INSTALLATION.)

4. Verify the continuity between parking sensor buzzer terminals A and B.

ac9wzw00002678

  • If not as indicated in the table, replace the parking sensor buzzer.

  ac5wzw00005599