DRIVE BELT AUTO TENSIONER INSPECTION [MZI-3.7]

id0110c5801700

1. Remove the engine cover. (See ENGINE COVER REMOVAL/INSTALLATION [MZI-3.7].)

2. Remove the front wheel and tire (RH). (See GENERAL PROCEDURES (SUSPENSION).)

3. Remove the splash shield (RH).

4. Remove the generator and A/C drive belt. (See DRIVE BELT REMOVAL/INSTALLATION [MZI-3.7].)

5. Verify that the drive belt auto tensioner moves smoothly in the operational direction.

  • Replace the drive belt auto tensioner if necessary.

ac9wzw00002214

  Tightening torque

  8.9—12.1 N·m {91—123 kgf·cm, 79—107 in·lbf}

6. Turn the drive belt auto tensioner pulley by hand and verify that it rotates smoothly.

  • Replace the drive belt auto tensioner if necessary.

ac9wzw00002215

  Tightening torque

  8.9—12.1 N·m {91—123 kgf·cm, 79—107 in·lbf}

7. Install in the reverse order of removal.