BASS-BOX REMOVAL/INSTALLATION

id092000815200

1. Disconnect the negative battery cable.

2. Remove the trunk box. (See TRUNK BOX REMOVAL/INSTALLATION.)

3. Remove the seat side box. (See SEAT SIDE BOX REMOVAL/INSTALLATION.)

4. Remove the trunk end trim. (See TRUNK END TRIM REMOVAL/INSTALLATION.)

5. Remove in the order indicated in the table.

ac9uuw00000399

1 | Connector
2 | Nut
3 | Bass-box cover
4 | Bass-box

6. Install in the reverse order of removal.