TRANSAXLE RANGE (TR) SWITCH OPERATION [AY6A-EL, AY6AX-EL]

id0517k3223900

• A non-contact type TR switch has been adopted in the TCM. The TR switch detects shift position by using the Hall Effect, which outputs specified voltage according to the shift position (P, R, N, D). Compared to the contact type switch, the non-contact type switch does not have contact points and is very compact. This makes it possible to integrate it with the TCM, improving reliability and durability.

ac9uun00000845