DRIVE INFORMATION SYSTEM CONSTRUCTION

id092200111300

Instant Update Fuel Economy Mode

• Instant update fuel economy is calculated from the trip distance and the fuel consumption in the previous 2 s.
• Instrument fuel economy is updated from every 2 s (indication only changes when difference between present value and next value is 0.8 L/100 km or more).

Calculation
  ― Instant fuel economy (L/100km)= Fuel consumption over last 2 s (L) / Distance travelled over last 2 s (km)×100

• When fuel is not consumed, for example, when applying an engine brake, <0.0 L/100 km> is displayed.
• When the vehicle speed is in the invalid display range (see the following chart), <---/100 km> is displayed.

ac9wzn00000533

Average Fuel Economy Mode

• Average fuel economy is calculated from the trip distance and the fuel consumption from the time when the battery is last connected or the average fuel economy data is reset.
• Average fuel economy is updated every 1 min.

Calculation
  ― Average fuel economy (L/100 km)= Cumulative fuel consumption (L) / Cumulative trip distance (km) × 100

• When the cumulative trip distance is 0 km (vehicle has not traveled since battery was last connected or average fuel economy function was last reset), <99.9 L/100 km> is displayed.
• When the INFO button is pressed for 1 s or more while displaying the average fuel economy, the cumulative fuel consumption data and cumulative trip distance data are reset.
• After the data are reset, <--- L/100 km> is displayed for 1 min.

Remaining Possible Travel Distance Mode

• Remaining possible travel distance is calculated from the past 0.1 km interval fuel consumption (L/km), the cumulative fuel consumption (L/km), and the remaining travel quantity (L).

Calculation
  ― Remaining travel distance (km)= Remaining fuel quantity (L) / Cumulative fuel consumption (L/km) + Past 0.1 km interval fuel consumption (L/km)

• Remaining possible travel distance is updated every 1 s.

Average Vehicle Speed Mode

• Average vehicle speed is calculated from the distance driven and the specified time from the time the battery is last connected or the average vehicle speed data is last reset.
• Average vehicle speed is updated every 10 s.

Calculation
  ― Average vehicle speed (km/h)= Cumulative distance driven (km) / Cumulative specified time (hour)

• When the INFO button is pressed for 1 s or more while displaying the average vehicle speed, the cumulative distance driven data and the cumulative specified time data are reset.
• After the data are reset, <--- km/h> is displayed for 1 min.