COLUMN COVER REMOVAL/INSTALLATION

id091700800800

Lower Column Cover

1. Remove the screws.

ac9uuw00000340

2. Pull down the tilt wheel release lever.

3. Remove the lower column cover in the direction of the arrow.

4. Install in the reverse order of removal.

Upper Column Cover Removal

1. Pull the upper column cover upward and detach the upper column cover from the lower column cover.

ac9wzw00003019

2. Push the rubber in the direction of the arrow while pinching part A of the rubber.

ac9uuw00002138

  Caution
  • Remove the rubber by pressing it from the backside of the upper column cover. The rubber may deform if it is pulled forcibly or pried with a flathead screwdriver.

3. Push the rubber in the direction of the arrow while partially peeling part B of the rubber.

ac9uuw00002139

4. Push part C of the rubber in the direction of the arrow and remove the upper column cover.

ac9uuw00002140

5. Install in the reverse order of removal.

Upper Column Cover Installation

1. Push the rubber in the direction of the arrow in the order of A, B, and C part to install the upper column cover to the rubber.

ac9uuw00002262

2. Install the upper column cover to the lower column cover.