POWER STEERING OIL PUMP REMOVAL/INSTALLATION [L.H.D.]

id0614008007d3

1. Remove the windshield wiper arm and blade. (See WINDSHIELD WIPER ARM AND BLADE REMOVAL/INSTALLATION.)

2. Remove the cowl grill. (See COWL GRILLE REMOVAL/INSTALLATION.)

3. Remove the windshield wiper motor (See WINDSHIELD WIPER MOTOR REMOVAL/INSTALLATION.)

4. Remove the cowl panel. (See COWL PANEL REMOVAL/INSTALLATION.)

5. Remove the right side splashing shield.

6. Remove the drive belt. (See DRIVE BELT REMOVAL/INSTALLATION [MZI-3.7].)

7. Remove in the order indicated in the table.

8. Install in the reserve order of removal.

ac9wzw00000701

1 | Pressure switch connector
2 | Pressure pipe
3 | Bolts
4 | Suction hose clamp (Power steering fluid tank side)
5 | Power steering oil pump and suction hose
6 | Suction hose
7 | Power steering oil pump (See Power Steering Oil Pump Removal Note.)
8 | Return hose clamp
9 | Return hose
10 | Power steering fluid tank (See Power Steering Fluid Tank Removal Note.)

Power Steering Oil Pump Removal Note

1. Remove the power steering oil pump upward.

Power Steering Fluid Tank Removal Note

1. Remove the coolant reserve tank with the hose still connected, and position the coolant reserve tank out of the way.

ac9uuw00001653