OUTER MIRROR GARNISH REMOVAL

id091200003100

1. Remove the outer mirror glass from the outer mirror. (See OUTER MIRROR GLASS REMOVAL.)

2. Pinch the clip ends using pincers and detach the clips by pushing them forward.

ac9wzw00001665

3. Pull the upper side of outer mirror garnish in the direction of the arrow (1) shown in the figure.

ac9wzw00000505

4. Pull the lower side of outer mirror garnish in the direction of the arrow (2) shown in the figure and remove it while detaching clips.

ac9wzw00000506

5. Remove the outer mirror garnish.