ROOM LIGHT CONTROL SYSTEM OPERATION

id091800101200

Conditions before operation (Conditions which must be satisfied) | Operation condition | Interior light | Cancel condition (When any condition satisfied)
--- | --- | --- | ---
Illumination time | Brightness
• Turn the ignition switch to the OFF or ACC position. • All doors are closed. (All door switches off) | Any door open. (Any door switch on) | Approx. 30 min | 100 % | • All doors are closed except liftgate. (All door switches off) • After illumination time.*1
• Key extracted from steering lock. (Key reminder switch is off.) • All doors are closed. (All door switches off) • Driver’s door lock knob is locked. (Door lock-link switch is in lock position.) | Driver’s door lock knob is unlocked. (Door lock-link switch is in unlock position.) | Approx. 30 s | 100 % | • Turn the ignition switch to the ON position. • Any door open. (Any door switch on) • Driver’s door lock knob is locked. (Door lock-link switch is in lock position.) • After illumination time.
• Key inserted into steering lock. (Key reminder switch is on.) • All doors are closed. (All door switches off) | Key extracted from steering lock. (Key reminder switch is off.) | Approx. 15 s | 100 % | • Turn the ignition switch to the ON position. • Any door open. (Any door switch on) • Driver’s door lock knob is locked. (Door lock-link switch is in lock position.) • After illumination time.
• Turn the ignition switch to the OFF or ACC position. • Any door is open. (Any door switches on) • Driver’s door lock knob is unlocked. (Door lock-link switch is in unlock position.) | All doors are closed. (All door switches off) | Approx. 15 s | 60 % | • Turn the ignition switch to the ON position. • Any door open. (Any door switch on) • Driver’s door lock knob is locked. (Door lock-link switch is in lock position.) • After illumination time.

*1 :After interior light is turned off according to this cancel condition, the light will illuminate again when either of the following conditions are satisfied:
• After all doors are closed, then any door is reopened.
(After all door switches are off, any door switch is on)
• After all doors are closed, then ignition switch is at the ON position. (Ignition switch ON)

ac9wzn00000583