DSC/RSC HU AIR BLEEDING

id041800816500

1. Turn the ignition switch to the OFF position.

2. Connect the M-MDS to the DLC-2.

ac9uuw00000862

3. After the vehicle is identified, select the following items from the initialization screen of the M-MDS.

  • When using the IDS (laptop PC)
    1. Select “Chassis”.
    2. Select “Braking”.

  • When using the PDS (Pocket PC)
    1. Select “All Tests and Calibrations”.

4. Then, select items from the screen menu in the following order.

  • Select “ABS Service Bleed”

5. Perform the air bleeding according to the directions on the screen.