AUDIO AMPLIFIER REMOVAL/INSTALLATION

id092000801100

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Trunk box (See TRUNK BOX REMOVAL/INSTALLATION.)

  (2) Seat side box (RH) (See SEAT SIDE BOX REMOVAL/INSTALLATION.)

  (3) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (4) Third-row seat (RH) (See THIRD-ROW SEAT REMOVAL/INSTALLATION.)

  (5) Rear scuff plate inner (RH) (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)

  (6) Third-row seat belt lower anchor installation bolt (RH) (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (7) Trunk side trim (RH) (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

ac9uuw00000698

1 | Connector
2 | Nut
3 | Audio amplifier

4. Install in the reverse order of removal.

5. Perform the audio amplifier configuration after replacing the audio amplifier. (See AUDIO AMPLIFIER CONFIGURATION.)

  Caution
  • Perform the audio amplifier configuration after replacing the audio amplifier to assure that the audio system operates correctly.