POWER OUTER MIRROR OPERATION

id091200007300

Mirror Glass Adjustment

• The left/right selection switch establishes left or right side outer mirror circuit and current is supplied in either one of the four directions according to the position of the mirror glass adjustment switch. Due to this, the motor rotates either up or down, left or right.

Ex.) Left side outer mirror is moved upward

1. When the mirror glass adjustment switch is pressed, the outer mirror glass adjustment signal is input to the position memory control module.

2. When the outer mirror glass adjustment signal is input, the position memory control module turns on the TR1 and TR2 to operate the power outer mirror.

With position memory system

ac9wzn00000270

Without position memory system

acxuun00000526

Retract/return

1. When the retractable outer mirror switch is moved to the retract position, a circuit is established, and the retract/return motor rotates in the retracting direction.

2. During return operation, the motor rotates in the opposite (returning) direction.

ac9wzn00000993