DTC 95

id070200805000

DTC 95 | Rear air mix actuator (motor lock) (past)
--- | ---
POSSIBLE CAUSE | • Rear air mix actuator malfunction • Rear A/C unit (air mix link and/or air mix crank) malfunction • Open or short circuit between rear air mix actuator and front climate control unit

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Disconnect rear air mix actuator connector. • Connect battery positive voltage to terminal F (or terminal G) and ground to terminal G (or terminal F) of rear air mix actuator connector. • Does rear air mix actuator operate? | Yes | Connect rear air mix actuator connector, then go to Step 3.
No | Go to the next step.
2 | • Remove rear air mix actuator. (See REAR AIR MIX ACTUATOR REMOVAL/INSTALLATION.) • Operate air mix link by hand. • Does air mix link operate smoothly? | Yes | Replace rear air mix actuator.
No | Replace air mix link and/or air mix crank.
3 | • Disconnect front climate control unit connector (24-pin). • Connect battery positive voltage to terminal 1I (or terminal 1G) and ground to terminal 1G (or terminal 1I) of front climate control unit connector (24-pin). • Does rear air mix actuator operate? | Yes | Inspect the connection of the front climate control unit connector.
No | Repair wiring harness.