ENGINE OIL LEVEL INSPECTION [MZI-3.7]

id0111e3800500

1. Position the vehicle on level ground.

2. Warm up the engine.

3. Stop the engine and allow at least 5 min before continuing.

4. Remove the dipstick, wipe it cleanly, and reinstall it fully.

5. Remove the dipstick and verify that the oil level is between the L and F marks on the dipstick.

ac9wzw00001045

  • If the oil level is below the L mark, add to raise the level within the hatching zone.