DTC TABLE [Bluetooth SYSTEM (HANDS-FREE TELEPHONE (HF/TEL) SYSTEM)]

id0902g8855700

— :Not applicable

DTC | Security indicator light | Description | Fail-safe | Drive cycle | Self-test type*1 | Memory function | Reference
--- | --- | --- | --- | --- | --- | --- | ---
Method using M-MDS | On-board diagnostic test mode
— | 26:Er81 | — | Communication error with audio unit | — | — | D | — | (See DTC: U0197:00, 26:Er81 [Bluetooth SYSTEM (HANDS-FREE TELEPHONE (HF/TEL) SYSTEM)].)
B116A:12 | 26:Er82 | — | Open circuit in microphone circuit | — | — | D | — | (See DTC: B116A:12, 26:Er82 [Bluetooth SYSTEM (HANDS-FREE TELEPHONE (HF/TEL) SYSTEM)].)
B116A:13 | —*2 | — | Open circuit in microphone circuit | — | — | D | — | (See DTC: B116A:13 [Bluetooth SYSTEM (HANDS-FREE TELEPHONE (HF/TEL) SYSTEM)].)
B116A:44 | 26:Er86 | — | Bluetooth unit internal malfunction | — | — | D | — | (See DTC: B116A:44, 26:Er86 [Bluetooth SYSTEM (HANDS-FREE TELEPHONE (HF/TEL) SYSTEM)].)
U0197:00 | —*2 | — | Communication error with audio unit | — | — | D | — | (See DTC: U0197:00, 26:Er81 [Bluetooth SYSTEM (HANDS-FREE TELEPHONE (HF/TEL) SYSTEM)].)
— | —*2 | — | DTCs not stored | — | — | — | — | —

*1 :D: ODDTC self test
*2 :It is not displayed in the audio display because the on-board diagnostic test mode is not available.