DTC U0534:68 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE]

id0902q2393400

Description | Error signal from BSM control module (RH)
--- | ---
Detection condition | • BSM control module (LH) receives the error signal from the BSM control module (RH) for 1 s or more.
Possible cause | • BSM control module (RH) malfunction • BSM control module (LH) malfunction

Diagnostic procedure

Step | Inspection | Action
--- | --- | ---
1 | PERFORM DTC INSPECTION AND VERIFY BSM CONTROL MODULE (RH) MALFUNCTION • Clear the DTC for the BSM control module (LH) using the M-MDS. (See CLEARING DTC [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].) • Retrieve the BSM control module (LH) DTCs using the M-MDS. (See DTC INSPECTION [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].) • Is the same DTC displayed? | Yes | Replace the BSM control module (RH), then go to the next step. (See BLIND SPOT MONITORING (BSM) CONTROL MODULE REMOVAL/INSTALLATION [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].)
No | Go to Step 3.
2 | VERIFY DTC TROUBLESHOOTING COMPLETED • Clear the DTC for the BSM control module (LH) using the M-MDS. (See CLEARING DTC [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].) • Retrieve the BSM control module (LH) DTCs using the M-MDS. (See DTC INSPECTION [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].) • Is the same DTC displayed? | Yes | Repeat the inspection from Step 1. • If the malfunction recurs, replace the BSM control module (LH). (See BLIND SPOT MONITORING (BSM) CONTROL MODULE REMOVAL/INSTALLATION [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].) Go to the next step.
No | Go to the next step.
3 | VERIFY IF OTHER DTCs DISPLAYED • Are any other DTCs displayed? | Yes | Repair or replace the malfunctioning part according to the applicable DTC troubleshooting. (See DTC TABLE [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].)
No | DTC troubleshooting completed.