CLEARING DTC [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE]

id0902q3960400

CMDTC Memory Clearing Procedure

1. Connect the M-MDS to the DLC-2.

ac9uuw00002673

2. After the vehicle is identified, select the following items from the initialization screen of the M-MDS.

  (1) Select “Self Test”.

  (2) Select “All CMDTCs”.

3. Verify the DTC according to the directions on the screen.

4. Press the clear button on the DTC screen to clear the DTC.

5. Switch the ignition off.

6. Switch the ignition ON (engine off or on) and wait for 5 s or more.

7. Perform DTC inspection. (See DTC INSPECTION [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)

8. Verify that no DTCs are displayed.

ODDTC Memory Clearing Procedure

1. Connect the M-MDS to the DLC-2.

ac9uuw00002673

2. After the vehicle is identified, select the following items from the initialization screen of the M-MDS.

  (1) Select “Self Test”.

  (2) Select “Modules”.

  (3) Select “BSML” or “BSMR”.

3. Verify the DTC according to the directions on the screen.

4. Press the clear button on the DTC screen to clear the DTC.

5. Switch the ignition off.

6. Switch the ignition ON (engine off or on) and wait for 5 s or more.

7. Perform DTC inspection. (See DTC INSPECTION [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)

8. Verify that no DTCs are displayed.