DTC B266A [POWER LIFTGATE (PLG) SYSTEM]

id0902e9381300

DTC B266A | Rotation sensor circuit malfunction
--- | ---
DETECTION CONDITION | A short circuit to ground in the PLG drive unit (rotation sensor) continues for 5 min or more.
POSSIBLE CAUSE | • Short to GND in wiring harness between PLG control module terminal 2K and PLG drive unit terminal E • Rotation sensor malfunction • PLG control module malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT WIRING HARNESS BETWEEN PLG CONTROL UNIT AND PLG DRIVE UNIT • Disconnect the PLG control module connector. • Disconnect the PLG drive unit connector. • Inspect the wiring harness between PLG control module terminal 2K and PLG drive unit terminal E for a short circuit to ground system. | Yes | Replace the PLG drive unit. (See POWER LIFTGATE (PLG) DRIVE UNIT REMOVAL/INSTALLATION.) Go to the next step.
No | Repair or replace the wiring harness. Go to the next step.
2 | VERIFY CORRECTION COMPLETED • Reconnect the disconnected connector. • Clear the DTC. • Is DTC B266A stored after 5 min or more have elapsed? | Yes | Replace the PLG control module. (See POWER LIFTGATE (PLG) CONTROL MODULE REMOVAL/INSTALLATION.)
No | DTC troubleshooting completed.