CLEARING DTC [THEFT-DETERRENT SYSTEM]

id0902g7960400

1. Connect the M-MDS (IDS) to the DLC-2.

ac9uuw00000452

2. After the vehicle is identified, select the following items from the initialization screen of the IDS.

  (1) Select “Self Test”.

  (2) Select “Modules”.

  (3) Select “VSM”.

3. Verify the DTC according to the directions on the screen.

4. Press the clear button on the DTC screen to clear the DTC.

5. Turn the ignition switch to the OFF position.

6. Turn the ignition switch to the ON position and wait for 5 s or more.

7. Perform DTC inspection. (See DTC INSPECTION [THEFT-DETERRENT SYSTEM].)

8. Verify that no DTCs are displayed.