ON-BOARD DIAGNOSIS SYSTEM (THEFT-DETERRENT SYSTEM) MALFUNCTION DIAGNOSIS FUNCTION [WITH INTRUDER SENSOR]

id0914000047b7

On-board Diagnostic Function

Malfunction detection function

  • Detects overall malfunctions in the theft-deterrent system-related parts.

Display function

  • If any malfunction is detected, the security light in the instrument cluster illuminates to inform the driver of a system malfunction.

Memory function

  • Stores malfunctions in the theft-deterrent system-related parts detected by the malfunction detection function, and the stored malfunction contents are not cleared even if the ignition switch is turned to the OFF position or the negative battery cable is disconnected.

DTC table

DTC | Description
--- | ---
M-MDS display
B109F:49 | Intruder sensor internal malfunction
B109F:86 | Signal error from intruder sensor
B109F:87 | Communication error between intruder sensor and theft-deterrent control module
B10A5:49 | Theft-deterrent siren internal malfunction
B10A5:86 | Signal error from theft-deterrent siren
B10A5:87 | Communication error between theft-deterrent siren and theft-deterrent control module
B1174:13 | Door lock-link switch (passenger-side/LR/RR) circuit malfunction
P254F:13 | Bonnet latch switch circuit malfunction
U0001:88 | Module communication error (HS-CAN)
U0100:00 | Communication error with PCM
U0300:00 | Configuration error
U2100:00
U3000:49 | Theft-deterrent control module internal malfunction
U3003:16 | Theft-deterrent control module power supply circuit malfunction
U3003:17