BSM OFF INDICATOR LIGHT DOES NOT ILLUMINATE WHEN THE IGNITION IS SWITCHED TO ON [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE]

id0903n2015000

Description | BSM OFF indicator light does not illuminate when the ignition is switched to ON
• BSM OFF indicator light does not illuminate when the ignition is switched to ON. • The BSM control module does not communicate with the M-MDS.
Possible Causes | • BSM control module (LH) does not initiate ― Open or short circuit in BSM control module (LH) power supply circuit (open or short to power supply circuit in wiring harness between push button start and BSM control module (LH) terminal I) ― Open circuit in BSM control module (LH) ground circuit (open circuit in wiring harness between BSM control module (LH) and ground, poor contact at ground point) ― BSM control module (LH) malfunction • Instrument cluster does not illuminate BSM OFF indicator light ― Instrument cluster malfunction

Diagnostic Procedure

Step | Inspection | Result | Action
--- | --- | --- | ---
1 | INSPECT BSM CONTROL MODULE (LH) POWER SUPPLY VOLTAGE • Switch the ignition ON (engine off or on). • Measure the voltage at BSM control module (LH) terminal I. • Is the voltage B+? | Yes | Go to the next step.
No | Inspect and repair for the following: • Inspect the condition of fuses between the push button start and the BSM control module (LH), and perform repairs at the location where the fuse is blown. • Refer to the wiring diagram and verify whether or not there is a common connector between the push button start and the BSM control module (LH). If there is a common connector: ― Determine the malfunctioning part by inspecting the common connector and the terminal for corrosion, damage, or pin disconnection, and the mid-wiring harness for a open circuit. ― Repair or replace the wiring harness. If there is no common connector: ― Repair or replace the wiring harness.
2 | INSPECT BSM CONTROL MODULE (LH) GROUND CIRCUIT • Switch the ignition off (LOCK). • Verify that there is continuity between the BSM control module (LH) terminal J and ground. • Is there continuity? | Yes | Go to the next step.
No | Inspect and repair the ground point. Repair or replace for an open circuit between the BSM control module (LH) and ground.
3 | INSPECT IF MALFUNCTION IS IN INSTRUMENT CLUSTER OR BSM CONTROL MODULE (LH) • Turn on the BSM OFF indicator light using check code 26 of the instrument cluster input/output check mode function. (See INSTRUMENT CLUSTER INPUT/OUTPUT CHECK MODE.) • Does the BSM OFF indicator light illuminate? | Yes | Replace the BSM control module (LH). (See BLIND SPOT MONITORING (BSM) CONTROL MODULE REMOVAL/INSTALLATION [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
No | Replace the instrument cluster (See INSTRUMENT CLUSTER REMOVAL/INSTALLATION.)