FOW/LDWS SWITCH INSPECTION

id092200035200

1. Disconnect the negative battery cable.

2. Remove the FOW/LDWS switch. (See FOW/LDWS SWITCH REMOVAL/INSTALLATION.)

3. Verify that the continuity is as indicated in the table.

ac9wzw00002631

  • If not as indicated in the table, replace the cluster switch.

4. Apply battery positive voltage to FOW/LDWS switch terminal E, and connect terminal A to ground.

ac9wzw00002682

5. Verify that the LED illuminates.

  • If there is any malfunction, replace the cluster switch.