PID/DATA MONITOR TABLE [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE]

id0902q3960700

BSM Control Module (LH)

—: Not applicable

PID | Unit/Operation | Data contents | Module control terminal
--- | --- | --- | ---
DTC_CNT | — | Displays number of DTCs stored in the BSM control module (LH) | —
IL_MODE | Off/On | • Off: BSM OFF indicator light is illuminated in night mode. • On: BSM OFF indicator light is illuminated in daytime mode. | C, D (CAN)
RCTA_BUZZER | Off/On | • Off: RCTA warning alarm does not sound. • On: RCTA warning alarm sounds. | C, D (CAN)
RCTA_OFF_IL | Off/On | • Off: BSM OFF indicator light is not illuminated. • On: BSM OFF indicator light is illuminated. | C, D (CAN)
RCTA_WARN | Off/On | • Off: BSM indicator lights are not illuminated. • On: BSM indicator lights are illuminated. Note • BSM indicator lights will be turned on, if the selector lever is in R position. | C, D (CAN)
SHIFT_R | Not_R/R | • Not_R: Selector lever is in position other than R. • R: Selector lever is in R position. | C, D (CAN)
SWA_POS | ° (deg) | Displays steering angle signal (estimated absolute angle) • Steering wheel in neutral position: Near 0 degrees • Steering wheel turned to left: Changes from 0 degrees to positive • Steering wheel turned to right: Changes from 0 degrees to negative | C, D (CAN)
VPWR_IG1 | V | Displays BSM control module (LH) power supply voltage | I (Power supply)
VSPD | KPH, MPH | Displays vehicle speed | C, D (CAN)
WRN_IND_L | Off/On | • Off: BSM indicator light (LH) is not illuminated. • On: BSM indicator light (LH) is illuminated. | • G (BSM indicator light (LH) signal) • J (Ground)

BSM Control Module (RH)

—: Not applicable

PID | Unit/Operation | Data contents | Module control terminal
--- | --- | --- | ---
DTC_CNT | — | Displays number of DTCs stored in the BSM control module (RH) | —
IL_MODE | Off/On | • Off: BSM OFF indicator light is illuminated in night mode. • On: BSM OFF indicator light is illuminated in daytime mode. | A, B (CAN)
RCTA_OFF_IL | Off/On | • Off: BSM OFF indicator light is not illuminated. • On: BSM OFF indicator light is illuminated. | A, B (CAN)
SHIFT_R | Not_R/R | • Not_R: Selector lever is in position other than R. • R: Selector lever is in R position. | A, B (CAN)
SWA_POS | ° (deg) | Displays steering angle signal (estimated absolute angle) • Steering wheel in neutral position: Near 0 degrees • Steering wheel turned to left: Changes from 0 degrees to positive • Steering wheel turned to right: Changes from 0 degrees to negative | A, B (CAN)
VPWR_IG1 | V | Displays BSM control module (RH) power supply voltage | I (Power supply)
VSPD | KPH, MPH | Displays vehicle speed | A, B (CAN)
WRN_IND_R | Off/On | • Off: BSM indicator light (RH) is not illuminated. • On: BSM indicator light (RH) is illuminated. | • G (BSM indicator light (RH) signal) • J (Ground)