PID/DATA MONITOR TABLE [POWER LIFTGATE (PLG) SYSTEM]

id0902e9345900

PID name (definition) | Unit/Condition | Operation Condition (Reference)
--- | --- | ---
DTC_CNT (Number of continuous DTCs) | — | Indicates number of DTC
LAT_FULL (Liftgate latch and lock actuator (full latch switch)) | Off / On | • Full latch switch on: on • Other: off
LAT_HALF (Liftgate latch and lock actuator (half latch switch)) | Off / On | • Half latch switch on: on • Other: off
LAT_RTN (Liftgate latch and lock actuator (return switch)) | Off / On | • Return switch on: on • Other: off
MTR_CLS_CL (Closure motor (CLOSE)) | Off / On | • Closure motor (CLOSE) operation: on • Other: off
MTR_CLS_OP (Closure motor (OPEN)) | Off / On | • Closure motor (OPEN) operation: on • Other: off
MTR_PLG_C (PLG motor current) | A | • Voltage: Refer to graph 1 Note • The values in the graph are a reference showing the relation between the elapsed period and voltage. The values change according to vehicle conditions/status, temperature, and battery voltage.
MTR_PLG_CL (PLG motor (CLOSE)) | Off / On | • PLG motor (CLOSE) operation: on • Other: off
MTR_PLG_OP (PLG motor (OPEN)) | Off / On | • PLG motor (OPEN) operation: on • Other: off
PWR_IG1 (Ignition 1 (IG1) electric source) | Off / On | • Ignition switch is at ON: on • Other: off
SW_CCL (Liftgate latch switch) | Off / On | • Unlatch (liftgate is open): on • Latch (liftgate is closed): off
SW_MAIN (PLG front switch) | Off / On | • PLG front switch on position: on • Other: off
SW_SUB (PLG rear switch) | Off / On | • PLG rear switch on position: on • Other: off
TCH_L_FLT (PLG touch sensor (LH) failure) | O.K. / Fault | • PLG touch sensor (LH) normal: O.K. • PLG touch sensor (LH) malfunction: Fault
TCH_L_ST (PLG touch sensor (LH) condition) | Off / On | • PLG touch sensor (LH) on: on • Other: off
TCH_L_V (PLG touch sensor (LH) voltage) | V | Normal with no obstruction: 2.5 V
TCH_R_FLT (PLG touch sensor (RH) failure) | O.K. / Fault | • PLG touch sensor (RH) normal: O.K. • PLG touch sensor (RH) malfunction: Fault
TCH_R_ST (PLG touch sensor (RH) condition) | Off / On | • PLG touch sensor (RH) on: on • Other: off
TCH_R_V (PLG touch sensor (RH) voltage) | V | Normal with no obstruction: 2.5 V
VPWR (Module supply voltage) | V | Under any condition: VB

ac9uuw00002344