POWER LIFTGATE (PLG) SLIDER REMOVAL/INSTALLATION

id091100000700

  Note
  • The PLG drive unit has the following 2 types:
    ― Type A: PLG drive unit and PLG slider can be disassembled.
    ― Type B: Integrated PLG drive unit and PLG slider.

  ac9wzw00003044

TYPE A

  Note
  • If the negative battery cable is disconnected with the liftgate half opened, the clutch cannot be disengaged resulting in difficulty in opening/closing operation of the liftgate. Disconnect the negative battery cable with the liftgate in the fully open/close position.

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Trunk box (See TRUNK BOX REMOVAL/INSTALLATION.)

  (2) Seat side box (LH) (See SEAT SIDE BOX REMOVAL/INSTALLATION.)

  (3) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (4) Third-row seat (See THIRD-ROW SEAT REMOVAL/INSTALLATION.)

  (5) Third-row seat belt lower anchor installation bolt (LH) (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (6) Rear scuff plate inner (LH) (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)

  (7) Trunk side trim (LH) (See TRUNK SIDE TRIM REMOVAL/INSTALLATION)

  (8) Roof side trim (LH) (See ROOF SIDE TRIM REMOVAL/INSTALLATION.)

  (9) Third-row seat belt upper anchor installation bolt (LH) (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (10) D-pillar trim (LH) (See D-PILLAR TRIM REMOVAL/INSTALLATION.)

3. Disconnect the connection of the band that is on the PLG slider side of PLG arm with using the flat blade screwdriver.

ac9uuw00001731

4. Separate the PLG arm from the PLG slider.

5. Revolve the outer joint in the direction of the arrow to disconnect from the PLG slider and the PLG drive unit.

ac9wzw00001036

6. Remove the bolts.

7. Remove the PLG slider.

8. Install in the reverse order of removal.

TYPE B

  Note
  • If the negative battery cable is disconnected with the liftgate half opened, the clutch cannot be disengaged resulting in difficulty in opening/closing operation of the liftgate. Disconnect the negative battery cable with the liftgate in the fully open/close position.

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Trunk box (See TRUNK BOX REMOVAL/INSTALLATION.)

  (2) Seat side box (LH) (See SEAT SIDE BOX REMOVAL/INSTALLATION.)

  (3) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (4) Third-row seat (See THIRD-ROW SEAT REMOVAL/INSTALLATION.)

  (5) Third-row seat belt lower anchor installation bolt (LH) (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (6) Rear scuff plate inner (LH) (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)

  (7) Trunk side trim (LH) (See TRUNK SIDE TRIM REMOVAL/INSTALLATION)

  (8) Roof side trim (LH) (See ROOF SIDE TRIM REMOVAL/INSTALLATION.)

  (9) Third-row seat belt upper anchor installation bolt (LH) (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (10) D-pillar trim (LH) (See D-PILLAR TRIM REMOVAL/INSTALLATION.)

3. Disconnect the connection of the band that is on the PLG slider and drive unit side of PLG arm with using the flat blade screwdriver.

ac9wzw00003045

4. Put the PLG arm.

5. Remove the bolts.

ac9wzw00003046

6. Remove the PLG slider and drive unit.

7. Install in the reverse order of removal.