ANTENNA FEEDER NO.2 INSPECTION

id092000812500

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Front scuff plate inner (RH) (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)

  (2) Front side trim (RH) (See FRONT SIDE TRIM REMOVAL/INSTALLATION.)

  (3) Liftgate upper trim (See LIFTGATE UPPER TRIM REMOVAL/INSTALLATION.)

3. Disconnect the antenna feeder No.1. (See ANTENNA FEEDER NO.1 REMOVAL/INSTALLATION.)

4. Disconnect the antenna feeder No.2 connector. (See ANTENNA FEEDER NO.2 REMOVAL/INSTALLATION.)

5. Verify that the continuity between antenna feeder No.2 terminals is as indicated in the table.

ac9wzw00000899

  • If not as indicated in the table, replace antenna feeder No.2.

  ac9wzw00000900