ON-BOARD DIAGNOSTIC SYSTEM ACTIVE COMMAND MODES FUNCTION

id040200110700

• The active command modes function is used for optionally selecting active command modes items of input/output parts preset in the dynamic stability control (DSC)/roll stability control (RSC) hydraulic unit (HU)/control module (CM), and to operate them regardless of CM control.
• To protect the hydraulic unit interior, operate output related parts for only 10 s or less when using the active command modes function.

Active Command Modes Table

Command name | Output part name | Operation | Operation condition
--- | --- | --- | ---
PMP_MOTOR | Pump motor | Off/On | Ignition switch at ON
PWR_RLY | Valve relay
SSR_INTL | DSC/RSC sensor
V_LF_INL | LF inlet solenoid valve
V_LF_OTL | LF outlet solenoid valve
V_LR_INL | LR inlet solenoid valve
V_LR_OTL | LR outlet solenoid valve
V_RF_INL | RF inlet solenoid valve
V_RF_OTL | RF outlet solenoid valve
V_RR_INL | RR inlet solenoid valve
V_RR_OTL | RR outlet solenoid valve
V_STB_L | LH stability control solenoid valve
V_STB_R | RH stability control solenoid valve
V_TRC_L | LH traction control solenoid valve
V_TRC_R | RH traction control solenoid valve