AIR INTAKE ACTUATOR CONSTRUCTION

id074000101700

Construction

• Moves the air intake door based on the signals from the front climate control unit to switch between REC and FRESH.
• A sliding contact type has been adopted.

Operation

• Based on the signals from the front climate control unit, the motor in the air intake actuator operates to move the air intake door to the target position.
• When the door reaches the target position, the sliding junction turns off and the air intake door stops.

ac9wzn00000534