GENERAL PROCEDURES (FRONT AND REAR AXLES)

id031000800100

Wheel and Tire Installation

1. When installing the wheels and tires, tighten the wheel nuts in a criss-cross pattern to the following tightening torque.

  Tightening torque

  107.8—147.0 N·m {11.0—14.9 kgf·m, 79.6—108.4 ft·lbf}

Connector Disconnection

1. Disconnect the negative battery cable before performing any work that requires handling of connectors. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].)

Suspension Links Removal/Installation

1. For the joint sections with rubber bushings, raise the vehicle using a lift, and then temporarily tighten the installation bolts and nuts. Lower the vehicle to the ground and tighten them completely with the specified torque.

Electronic 4WD Control System Parts

1. After servicing the electronic 4WD control system parts, verify that no DTC has been stored. Clear any DTCs remaining in the memory. (See ELECTRONIC 4WD CONTROL SYSTEM ON-BOARD DIAGNOSIS.)

Auto Leveling System Initialization

1. Initialize the auto leveling sensor, when performing the following services. (See AUTO LEVELING SYSTEM INITIALIZATION.)

  ― Removing the auto leveling sensor
  ― Disconnecting the auto leveling sensor link
  ― Removing the suspension parts related the vehicle height