WASHER TANK REMOVAL/INSTALLATION

id091900801700

1. Disconnect the negative battery cable.

2. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

ac9wzw00001093

1 | Windshield washer motor connector
2 | Windshield washer hose
3 | Rear washer motor connector
4 | Rear washer hose
5 | Headlight cleaner control module (Vehicles with headlight cleaner)
6 | Bolt
7 | Washer tank
8 | headlight cleaner motor
9 | Washer fluid-level sensor (Vehicles with washer fluid-level sensor)

4. Install in the reverse order of removal.