NO.6 RECEPTION FREQUENCY OF RADIO SLIPS [RADIO]

id0903e3804800

6 | Reception frequency of radio slip
--- | ---
Possible DTC | Using the M-MDS | U3000:04
Without using M-MDS (On-board diagnostic test mode) | 09:Er22
Possible cause | • Electronic jamming from outside, or inferior condition of broadcasting station radio wave • Audio unit malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Push SEEK switch and check if desired broadcasting station is tuned. • Is it okay? | Yes | Go to Step 3.
No | Go to the next step.
2 | • Check if other broadcasting station is received at certain place when indication of reception frequency stays. • Is other station received? Note • When you receive weak signal from one broadcasting station and come close to broadcasting antenna which emits strong signal, broadcasting with strong signal is sometimes received. | Yes | Go to the next step.
No | Replace audio unit. (See AUDIO UNIT REMOVAL/INSTALLATION.)
3 | • Compare reception with other audio unit on same model (model/unit) under same problem conditions. • Is reception equivalent between customer’s unit and compared unit? | Yes | Troubleshooting completed.
No | Replace audio unit. (See AUDIO UNIT REMOVAL/INSTALLATION.)