POWER DOOR LOCK SYSTEM OPERATION

id091400191800

• The body control module (BCM) activates each lock actuator to lock/unlock according to the lock/unlock signal from the door lock switch.
• When the driver's door is locked/unlocked using the driver's door key cylinder, the door lock-link switch in the driver's door lock actuator is locked/unlocked via the rod.
• The body control module (BCM) activates each lock actuator to lock/unlock according to the lock/unlock signal from the door key cylinder switch.

ac9wzn00000976

Collision Detection Unlock Function Operation (With Collision Detection Unlock Function)

1. If a collision has occurred, the SAS control module sends a collision detection door unlock signal to the BCM (1).

2. The BCM unlocks all the doors after approx. 6 s it received the collision detection door unlock signal (2).

ac9wzn00001018