REAR BELTLINE MOLDING REMOVAL/INSTALLATION

id091600804700

Removal

1. Fully lower the rear door glass.

2. Remove the clip A using a protective tape-wrapped flathead screwdriver.

ac9wzw00001427

3. Lift (partially peeling back) the rear beltline molding in the direction of the arrow and then remove tabs B.

4. Remove the clip C.

5. Remove the rear beltline molding.

Installation

1. Install the clip A.

ac9wzw00001428

2. Install the tabs B.

3. Install the clip C.

4. Install the rear beltline molding.